NTi Press Release, 07 May 2019

New Features for the FX-Control Software
Good news for all FLEXUS FX100 customers! Version 3.0 of the FX-Control Software contains many new useful functions, and is available for free download.
A significant addition is in the field of electrical loudspeaker measurements. The calculation of the resonance frequency and the Thiele/Small parameters is now fully supported by the FX-Control software. These functions are available as a "calculation element" and fit seamlessly into the operating concept of the software. The impedance characteristics are used as input parameters, optionally with or without additional load on the loudspeaker membrane. The sequence control of the measurement is carried out in the FX-Control "Sequence mode", so it is possible to completely capture the electrical characteristics of a loudspeaker within a few seconds.
Another innovation is in the control of measurement sequences. The new "Continuous" option in the Sequence Editor, allows one measurement step to continuously execute until the user requests the next step. This makes it possible, for example, to carry out adjustment work on the test object during the measurement step.
As usual, the firmware and software updates for the FLEXUS FX100 are free. You can download Version 3.0 installation files and sample project files from the FLEXUS FX100 Support website.

Find this article on our website.